This plot shows the storm accumulated rainfall or the maximum rain rate at a point of interest (which, by default, is the center of the circular filter, if that is used; otherwise, the point can be specified when the routine is called), graphed as a function of the return period, which is the inverse of the annual probability of winds exceeding the value on the y axis. This quantity will depend on the wind profile selected in the params.m file.